**THE NEW TOYOTA PROACE CITY**

Specification Sheet

**ENGINE LINE UP**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Engine type | **PureTech S&S (EB2ADT)** | **PureTech S&S (EB2ADTS)** | **BlueHDi S&S (DV5RE)** | **BlueHDi S&S (DV5RD)** | **BlueHDi S&S (DV5RC)** | **BlueHDi S&S (DV5RC)** |
| Fuel | Petrol | Petrol | Diesel | Diesel | Diesel | Diesel |
| Displacement (cm3) | 1,199 | 1,199 | 1,499 | 1,499 | 1,499 | 1,499 |
| Max power (DIN hp/kW @ rpm) | 110hp/81kW @5500 | 130hp/96kW @5500 | 75hp/55kW @3500 | 100hp/75kW @3500 | 130hp/96kW @3750 | 130hp/96kW @3750 |
| Max torque (Nm @ rpm) | 205 N.m @1500 | 230 N.m @1600 | 210 N.m @1500 | 250 N.m @1700 | 300 N.m @1700 | 300 N.m @1700 |
| Transmission | Manual 6 speed | Robotized 8 speed | Manual 5 speed | Manual 5 speed | Manual 6 speed | Robotized 8 speed |
| C02 Emissions (combined g/km) | 124 | 123 | 109 | 108 | 118 | 114 |
| Fuel consumption (combined l/100 km) | 5.5 | 5.4 | 4.1 | 4.0 | 4.5 | 4.4 |
| Max speed (km/h) | 174 | 173 | 152 | 172 | 185 | 183 |
| Acc 0 to 100 km/h (seconds) | 11 | 9.8 | 15.8 | 11.5 | 9.8 | 10.6 |
| CV | ✔ | ✔ | ✔ | ✔ | ✔ | ✔ |
| PC | ✔ | ✔ | ✖ | ✔ | ✔ | ✔ |

**MAIN VEHICLE DIMENSIONS**

|  |  |  |
| --- | --- | --- |
| **PROACE CITY VAN** | | |
| Exterior dimensions (mm) | Short | Long |
| Overall length | 4,403 | 4,753 |
| Overall width (without mirror/mirrors deployed) | 1,848/2,107 | |
| Overall height (min./max.) | 1,796/1,860 | 1,812/1,860 |
| Wheelbase | 2,785 | 2,975 |
| Front track width | 1,548 - 1,563 | 1,553 |
| Rear track width | 1,568 - 1,577 | 1,549 - 1,568 |
| Front overhang | 892 | |
| Rear overhang | 726 | 886 |
| Ground clearance | 160 | 160 |
|  |  |  |
| Load compartment dimensions (mm) | Short | Long |
| Floor load length | 1,817 | 2,167 |
| Floor load length (with Smart Cargo) | 3,090 | 3,440 |
| Max. load compartment height | 1,200 - 1,270 | |
| Max. load width between sides (without/with 1/with 2 doors) | 1,733/1,630/1,527 | |
| Max. load width between wheels arches | 1,229 | |
| Load sill height (mini/maxi) | 547/625 | 560/617 |
| Sliding side door height | 1,072 | |
| Sliding side door width (with/without bulkhead) | 641 - 675/675 – 759 | |
| Rear door height | 1,196 | |
| Rear door width (lower section/upper section) | 1,241/1,087 | |
|  |  |  |
| Load compartment volume | Short | Long |
| Without Smart Cargo (m3) | 3.3 | 3.9 |
| With Smart Cargo (m3) | 3.8 | 4.3 |
| Number of Euro pallets | 2 | 2 |
|  |  |  |
| Masses and towing (kg) | Short | Long |
| Payload min./max.\* | 650/1,000 | 1,000 |
| Max. towing capacity\* | 1,500 | 1,500 |
| \* depending of the engine |  |  |

**MANOEUVRABILITY**

|  |  |  |
| --- | --- | --- |
|  | Short | Long |
| Turning circle between kerbs | 10,79 | 11,43 |
| Turning circle between walls | 11,29 | 11,93 |

|  |  |  |
| --- | --- | --- |
| **PROACE CITY VERSO** | | |
| Dimensions (mm) | Short | Long |
| Overall length | 4,403 | 4,753 |
| Overall width (without mirror/mirrors deployed) | 1,848/2,107 | |
| Overall height (without roof bar) | 1,800 | 1,812 |
| Wheelbase | 2,785 | 2,975 |
| Front track width | 1,553 | |
| Rear track width | 1,567 | |
| Front overhang | 892 | |
| Rear overhang | 726 | 886 |
| Ground clearance | 160 | 160 |
|  |  |  |
| Load compartment dimensions (mm) | Short | Long |
| Max. load length (passenger seatback retracted) | 2,700 | 3,050 |
| Max. load length behind row 1 | 1,880 | 2,230 |
| Max. load length behind row 2 | 1,000 | 1,350 |
| Max. load length behind row 3 | 236 | 418 - 566 |
| Boot width between wheel arches | 1,195 | |
| Max. load height | 1,126 | |
|  |  |  |
| Boot capacity  up to top of the seat/up to the roof (VDA litres) | Short | Long |
|
| - 5 seats | 597 - 641/983 | 850 - 912/1,538 |
| - 5 seats retracted row 2 | 1,414/2,126 | 1,672/2,693 |
| - 7 seats retracted row 3 | 571 | 806 |
| - 7 seats | 65 | 209 - 322 |